[Template:About](/wiki/Template:About" \o "Template:About) [Template:Pp-semi](/wiki/Template:Pp-semi) [Template:Pp-move-indef](/wiki/Template:Pp-move-indef) [Template:Use American English](/wiki/Template:Use_American_English) [Template:Use mdy dates](/wiki/Template:Use_mdy_dates) [Template:Infobox mineral](/wiki/Template:Infobox_mineral) **Diamond** ([Template:IPAc-en](/wiki/Template:IPAc-en) or [Template:IPAc-en](/wiki/Template:IPAc-en)) is a [metastable](/wiki/Metastable) [allotrope of carbon](/wiki/Allotropes_of_carbon), where the carbon [atoms](/wiki/Atoms) are arranged in a variation of the [face-centered cubic](/wiki/Face-centered_cubic) crystal structure called a [diamond lattice](/wiki/Diamond_lattice). Diamond is less [stable](/wiki/Chemical_stability) than [graphite](/wiki/Graphite), but the conversion rate from diamond to graphite is negligible at [standard conditions](/wiki/Standard_conditions_for_temperature_and_pressure). Diamond is renowned as a material with superlative physical qualities, most of which originate from the strong [covalent bonding](/wiki/Covalent_bond) between its atoms. In particular, diamond has the highest [hardness](/wiki/Scratch_hardness) and [thermal conductivity](/wiki/Thermal_conductivity) of any bulk material. Those properties determine the major industrial application of diamond in cutting and polishing tools and the scientific applications in [diamond knives](/wiki/Diamond_knife) and [diamond anvil cells](/wiki/Diamond_anvil_cell).

Because of its extremely rigid lattice, it can be contaminated by very few types of impurities, such as [boron](/wiki/Boron) and [nitrogen](/wiki/Nitrogen). Small amounts of defects or impurities (about one per million of lattice atoms) color diamond blue (boron), yellow (nitrogen), brown ([lattice defects](/wiki/Lattice_defect)), green (radiation exposure), purple, pink, orange or red. Diamond also has relatively high [optical dispersion](/wiki/Optical_dispersion) (ability to disperse light of different colors).

Most natural diamonds are formed at high temperature and pressure at depths of [Template:Convert](/wiki/Template:Convert) in the Earth's [mantle](/wiki/Mantle_(geology)). Carbon-containing minerals provide the carbon source, and the growth occurs over periods from 1 billion to 3.3 billion years (25% to 75% of the [age of the Earth](/wiki/Age_of_the_Earth)). Diamonds are brought close to the Earth's surface through deep [volcanic eruptions](/wiki/Volcanic_eruptions) by a [magma](/wiki/Magma), which cools into [igneous rocks](/wiki/Igneous_rock) known as [kimberlites](/wiki/Kimberlite) and [lamproites](/wiki/Lamproite). Diamonds can also be produced synthetically in a [HPHT method](/wiki/Synthetic_diamond#High_pressure,_high_temperature) which approximately simulates the conditions in the Earth's mantle. An alternative, and completely different growth technique is [chemical vapor deposition](/wiki/Chemical_vapor_deposition) (CVD). Several non-diamond materials, which include [cubic zirconia](/wiki/Cubic_zirconia) and [silicon carbide](/wiki/Silicon_carbide) and are often called [diamond simulants](/wiki/Diamond_simulants), resemble diamond in appearance and many properties. Special [gemological techniques](/wiki/Gemology) have been developed to distinguish natural diamonds, synthetic diamonds, and diamond simulants. The word is from the ancient [Greek](/wiki/Greek_language) ἀδάμας – *adámas* "unbreakable". [Template:Toclimit](/wiki/Template:Toclimit)

## Contents

* 1 History[[edit](/index.php?title=(none)&action=edit&section=1)]
  + 1.1 Natural history[[edit](/index.php?title=(none)&action=edit&section=2)]
    - 1.1.1 Formation in cratons[[edit](/index.php?title=(none)&action=edit&section=3)]
    - 1.1.2 Transport from mantle[[edit](/index.php?title=(none)&action=edit&section=4)]
    - 1.1.3 Space diamonds[[edit](/index.php?title=(none)&action=edit&section=5)]
* 2 Material properties[[edit](/index.php?title=(none)&action=edit&section=6)]
  + 2.1 Hardness[[edit](/index.php?title=(none)&action=edit&section=7)]
  + 2.2 Pressure resistance[[edit](/index.php?title=(none)&action=edit&section=8)]
  + 2.3 Electrical conductivity[[edit](/index.php?title=(none)&action=edit&section=9)]
  + 2.4 Surface property[[edit](/index.php?title=(none)&action=edit&section=10)]
  + 2.5 Chemical stability[[edit](/index.php?title=(none)&action=edit&section=11)]
  + 2.6 Color[[edit](/index.php?title=(none)&action=edit&section=12)]
  + 2.7 Identification[[edit](/index.php?title=(none)&action=edit&section=13)]
* 3 Industry[[edit](/index.php?title=(none)&action=edit&section=14)]
  + 3.1 Gem-grade diamonds[[edit](/index.php?title=(none)&action=edit&section=15)]
    - 3.1.1 Cutting[[edit](/index.php?title=(none)&action=edit&section=16)]
    - 3.1.2 Marketing[[edit](/index.php?title=(none)&action=edit&section=17)]
  + 3.2 Industrial-grade diamonds[[edit](/index.php?title=(none)&action=edit&section=18)]
  + 3.3 Mining[[edit](/index.php?title=(none)&action=edit&section=19)]
  + 3.4 Political issues[[edit](/index.php?title=(none)&action=edit&section=20)]
* 4 Synthetics, simulants, and enhancements[[edit](/index.php?title=(none)&action=edit&section=21)]
  + 4.1 Synthetics[[edit](/index.php?title=(none)&action=edit&section=22)]
  + 4.2 Simulants[[edit](/index.php?title=(none)&action=edit&section=23)]
  + 4.3 Enhancements[[edit](/index.php?title=(none)&action=edit&section=24)]
  + 4.4 Identification[[edit](/index.php?title=(none)&action=edit&section=25)]
* 5 Stolen diamonds[[edit](/index.php?title=(none)&action=edit&section=26)]
* 6 See also[[edit](/index.php?title=(none)&action=edit&section=27)]
* 7 References[[edit](/index.php?title=(none)&action=edit&section=28)]
* 8 Books[[edit](/index.php?title=(none)&action=edit&section=29)]
* 9 External links[[edit](/index.php?title=(none)&action=edit&section=30)]

## History[[edit](/index.php?title=(none)&action=edit&section=1)]

[Template:See also](/wiki/Template:See_also) The name *diamond* is derived from the ancient Greek *αδάμας* *(adámas*), "proper", "unalterable", "unbreakable", "untamed", from [ἀ-](/wiki/Wiktionary:ἀ-) (a-), "un-" + *δαμάω* (*damáō*), "I overpower", "I tame".[[1]](#cite_note-1) Diamonds are thought to have been first recognized and mined in India, where significant [alluvial deposits](/wiki/Alluvial_deposit) of the stone could be found many centuries ago along the rivers [Penner](/wiki/Penner_River), [Krishna](/wiki/Krishna_River) and [Godavari](/wiki/Godavari_River). Diamonds have been known in India for at least 3,000 years but most likely 6,000 years.<ref name=hershey> [Template:Cite book](/wiki/Template:Cite_book)</ref>

Diamonds have been treasured as gemstones since their use as [religious icons](/wiki/Icon) in [ancient India](/wiki/Kingdoms_of_Ancient_India). Their usage in engraving tools also dates to early [human history](/wiki/History_of_the_world).[[2]](#cite_note-2)<ref name=ancient\_China> [Template:Cite news](/wiki/Template:Cite_news)</ref> The popularity of diamonds has risen since the 19th century because of increased supply, improved cutting and polishing techniques, growth in the world economy, and innovative and successful advertising campaigns.<ref name=sell> [Template:Cite web](/wiki/Template:Cite_web)</ref>

In 1772, [Antoine Lavoisier](/wiki/Antoine_Lavoisier) used a lens to concentrate the rays of the sun on a diamond in an atmosphere of [oxygen](/wiki/Oxygen), and showed that the only product of the combustion was [carbon dioxide](/wiki/Carbon_dioxide), proving that diamond is composed of carbon.[[3]](#cite_note-3) Later in 1797, [Smithson Tennant](/wiki/Smithson_Tennant) repeated and expanded that experiment.[[4]](#cite_note-4) By demonstrating that burning diamond and graphite releases the same amount of gas, he established the chemical equivalence of these substances.<ref name=hazen/>

The most familiar uses of diamonds today are as gemstones used for [adornment](/wiki/Adornment), a use which dates back into antiquity, and as industrial abrasives for cutting hard materials. The [dispersion](/wiki/Dispersion_(optics)) of white light into [spectral colors](/wiki/Spectral_color) is the primary gemological characteristic of gem diamonds. In the 20th century, experts in gemology developed methods of grading diamonds and other gemstones based on the characteristics most important to their value as a gem. Four characteristics, known informally as the *four Cs*, are now commonly used as the basic descriptors of diamonds: these are [*carat*](/wiki/Carat_(unit)) (its weight), [*cut*](/wiki/Diamond_cut) (quality of the cut is graded according to [proportions](/wiki/Aspect_ratio), [symmetry](/wiki/Symmetry) and [polish](/wiki/Polishing)), [*color*](/wiki/Diamond_color) (how close to white or colorless; for fancy diamonds how intense is its hue), and [*clarity*](/wiki/Diamond_clarity) (how free is it from [inclusions](/wiki/Inclusion_(mineral))).[[5]](#cite_note-5) A large, flawless diamond is known as a [paragon](/wiki/Paragon_(diamond)).

### Natural history[[edit](/index.php?title=(none)&action=edit&section=2)]

The formation of natural diamond requires very specific conditions—exposure of carbon-bearing materials to high pressure, ranging approximately between 45 and 60 [kilobars](/wiki/Bar_(unit)) (4.5 and 6 [GPa](/wiki/Gigapascal)), but at a comparatively low temperature range between approximately [Template:Convert](/wiki/Template:Convert). These conditions are met in two places on Earth; in the [lithospheric mantle](/wiki/Lithosphere) below relatively stable [continental plates](/wiki/Continental_plate), and at the site of a meteorite strike.<ref name=core>[Template:Cite book](/wiki/Template:Cite_book)</ref>

#### Formation in cratons[[edit](/index.php?title=(none)&action=edit&section=3)]

[thumb|alt=A triangular facet of a crystal having triangular etch pits with the largest having a base length of about](/wiki/File:Diamond_face_trigons_scale.jpg) [Template:Convert](/wiki/Template:Convert)|One face of an uncut octahedral diamond, showing trigons (of positive and negative relief) formed by natural chemical etching The conditions for diamond formation to happen in the lithospheric mantle occur at considerable depth corresponding to the requirements of temperature and pressure. These depths are estimated between [Template:Convert](/wiki/Template:Convert) though occasionally diamonds have crystallized at depths about [Template:Convert](/wiki/Template:Convert).[[6]](#cite_note-6) The rate at which [temperature changes with increasing depth](/wiki/Geothermal_gradient) into the Earth varies greatly in different parts of the Earth. In particular, under oceanic plates the temperature rises more quickly with depth, beyond the range required for diamond formation at the depth required. The correct combination of temperature and pressure is only found in the thick, ancient, and stable parts of continental plates where regions of lithosphere known as [*cratons*](/wiki/Craton) exist. Long residence in the cratonic lithosphere allows diamond crystals to grow larger.[[6]](#cite_note-6) Through studies of carbon [isotope](/wiki/Isotope) ratios (similar to the methodology used in [carbon dating](/wiki/Carbon_dating), except with the [stable isotopes](/wiki/Stable_isotope) [C-12](/wiki/Carbon-12) and [C-13](/wiki/Carbon-13)), it has been shown that the carbon found in diamonds comes from both inorganic and organic sources. Some diamonds, known as [*harzburgitic*](/wiki/Peridotite), are formed from inorganic carbon originally found deep in the Earth's mantle. In contrast, [*eclogitic*](/wiki/Eclogite) diamonds contain organic carbon from organic [detritus](/wiki/Detritus) that has been pushed down from the surface of the Earth's [crust](/wiki/Crust_(geology)) through [subduction](/wiki/Subduction) (see [plate tectonics](/wiki/Plate_tectonics)) before transforming into diamond. These two different source of carbon have measurably different 13C:12C ratios. Diamonds that have come to the Earth's surface are generally quite old, ranging from under 1 [billion](/wiki/1000000000_(number)) to 3.3 billion years old. This is 22% to 73% of the age of the [Earth](/wiki/Earth).[[6]](#cite_note-6) Diamonds occur most often as [euhedral](/wiki/Euhedral) or rounded [octahedra](/wiki/Octahedron) and [twinned](/wiki/Crystal_twinning) octahedra known as *macles*. As diamond's crystal structure has a cubic arrangement of the atoms, they have many [facets](/wiki/Facet) that belong to a [cube](/wiki/Cube_(geometry)), octahedron, [rhombicosidodecahedron](/wiki/Rhombicosidodecahedron), [tetrakis hexahedron](/wiki/Tetrakis_hexahedron) or [disdyakis dodecahedron](/wiki/Disdyakis_dodecahedron). The crystals can have rounded off and unexpressive edges and can be elongated. Sometimes they are found grown together or form double "twinned" crystals at the surfaces of the octahedron. These different shapes and habits of some diamonds result from differing external circumstances. Diamonds (especially those with rounded crystal faces) are commonly found coated in *nyf*, an opaque gum-like skin.[[7]](#cite_note-7)

#### Transport from mantle[[edit](/index.php?title=(none)&action=edit&section=4)]

[right|thumb|float|220px|alt=Schematic cross section of an underground region 3 km deep and 2 km wide. A red dike stretches across the bottom, and a pipe containing some xenoliths runs from the dike to the surface, varying from red at the bottom to orange-yellow at the top. The pipe's root, at its bottom, is about 1 km long, and its diatreme, above the root, is about 1.5 km long. The pipe's top is a crater, rimmed by a tuff ring and containing washed-back ejecta. The erosion level is almost zero for Orapa, about 1 km for Jagersfontein, and about 1.4 km for Kimberley.|Schematic diagram of a volcanic pipe](/wiki/File:VolcanicPipe.jpg)

Diamond-bearing rock is carried from the mantle to the Earth's surface by deep-origin volcanic eruptions. The magma for such a volcano must originate at a depth where diamonds can be formed[[6]](#cite_note-6)—[Template:Convert](/wiki/Template:Convert) or more (three times or more the depth of source magma for most volcanoes). This is a relatively rare occurrence. These typically small surface volcanic craters extend downward in formations known as [volcanic pipes](/wiki/Volcanic_pipe).[[6]](#cite_note-6) The pipes contain material that was transported toward the surface by volcanic action, but was not ejected before the volcanic activity ceased. During eruption these pipes are open to the surface, resulting in open circulation; many [xenoliths](/wiki/Xenolith) of surface rock and even wood and fossils are found in volcanic pipes. Diamond-bearing volcanic pipes are closely related to the oldest, coolest regions of [continental crust](/wiki/Continental_crust) (cratons). This is because cratons are very thick, and their lithospheric mantle extends to great enough depth that diamonds are stable. Not all pipes contain diamonds, and even fewer contain enough diamonds to make mining economically viable.[[6]](#cite_note-6) The magma in volcanic pipes is usually one of two characteristic types, which cool into igneous rock known as either kimberlite or lamproite.[[6]](#cite_note-6) The magma itself does not contain diamond; instead, it acts as an elevator that carries deep-formed rocks (xenoliths), minerals ([xenocrysts](/wiki/Xenocryst)), and fluids upward. These rocks are characteristically rich in [magnesium](/wiki/Magnesium)-bearing [olivine](/wiki/Olivine), [pyroxene](/wiki/Pyroxene), and [amphibole](/wiki/Amphibole) minerals[[6]](#cite_note-6) which are often altered to [serpentine](/wiki/Serpentine_group) by heat and fluids during and after eruption. Certain *indicator minerals* typically occur within diamantiferous kimberlites and are used as mineralogical tracers by prospectors, who follow the indicator trail back to the volcanic pipe which may contain diamonds. These minerals are rich in [chromium](/wiki/Chromium) (Cr) or [titanium](/wiki/Titanium) (Ti), elements which impart bright colors to the minerals. The most common indicator minerals are chromium [garnets](/wiki/Garnet) (usually bright red chromium-[pyrope](/wiki/Pyrope), and occasionally green ugrandite-series garnets), eclogitic garnets, orange titanium-pyrope, red high-chromium [spinels](/wiki/Spinel), dark [chromite](/wiki/Chromite), bright green chromium-[diopside](/wiki/Diopside), glassy green olivine, black [picroilmenite](/wiki/Ilmenite), and [magnetite](/wiki/Magnetite). Kimberlite deposits are known as *blue ground* for the deeper serpentinized part of the deposits, or as *yellow ground* for the near surface [smectite](/wiki/Smectite) [clay](/wiki/Clay) and carbonate [weathered](/wiki/Weathering) and [oxidized](/wiki/Oxidation) portion.[[6]](#cite_note-6) Once diamonds have been transported to the surface by magma in a volcanic pipe, they may erode out and be distributed over a large area. A volcanic pipe containing diamonds is known as a *primary source* of diamonds. *Secondary sources* of diamonds include all areas where a significant number of diamonds have been eroded out of their kimberlite or lamproite [matrix](/wiki/Matrix_(geology)), and accumulated because of water or wind action. These include [alluvial](/wiki/Alluvium) deposits and deposits along existing and ancient shorelines, where loose diamonds tend to accumulate because of their size and density. Diamonds have also rarely been found in deposits left behind by glaciers (notably in [Wisconsin](/wiki/Wisconsin) and [Indiana](/wiki/Indiana)); in contrast to alluvial deposits, glacial deposits are minor and are therefore not viable commercial sources of diamond.[[6]](#cite_note-6)

#### Space diamonds[[edit](/index.php?title=(none)&action=edit&section=5)]

[Template:See also](/wiki/Template:See_also)

Not all diamonds found on Earth originated on Earth. Primitive interstellar meteorites were found to contain carbon possibly in the form of diamond.[[8]](#cite_note-8) A type of diamond called [carbonado](/wiki/Carbonado) that is found in South America and Africa may have been deposited there via an asteroid impact (not formed from the impact) about 3 billion years ago. These diamonds may have formed in the intrastellar environment, but as of 2008, there was no scientific consensus on how carbonado diamonds originated.<ref name=Garai2006> [Template:Cite journal](/wiki/Template:Cite_journal)</ref><ref name=Carbonardo> [Template:Cite web](/wiki/Template:Cite_web)</ref>

Diamonds can also form under other naturally occurring high-pressure conditions. Very small diamonds of micrometer and nanometer sizes, known as *microdiamonds* or [*nanodiamonds*](/wiki/Detonation_nanodiamond) respectively, have been found in meteorite [impact craters](/wiki/Impact_crater). Such impact events create shock zones of high pressure and temperature suitable for diamond formation. Impact-type microdiamonds can be used as an indicator of ancient impact craters.<ref name=core/> [Popigai crater](/wiki/Popigai_crater) in Russia may have the world's largest diamond deposit, estimated at trillions of carats, and formed by an asteroid impact.[[9]](#cite_note-9) Scientific evidence indicates that [white dwarf](/wiki/White_dwarf) stars have a core of crystallized carbon and oxygen nuclei. The largest of these found in the universe so far, [BPM 37093](/wiki/BPM_37093), is located [Template:Convert](/wiki/Template:Convert) away in the constellation [Centaurus](/wiki/Centaurus). A news release from the [Harvard-Smithsonian Center for Astrophysics](/wiki/Harvard-Smithsonian_Center_for_Astrophysics) described the [Template:Convert](/wiki/Template:Convert)-wide stellar core as a *diamond*.[[10]](#cite_note-10)

## Material properties[[edit](/index.php?title=(none)&action=edit&section=6)]

[Template:Main](/wiki/Template:Main) [thumb|left|Theoretically predicted](/wiki/File:Carbon_basic_phase_diagram.png) [phase diagram](/wiki/Phase_diagram) of carbon [thumb|alt=Four panels. First, seven clear faceted gems, six small and a large one. Second, black material with uneven surface. Third, three parallel atomic sheets, each resembling a chicken wire hedge. Fourth, a boxed atomic structure containing tetrahedrally arranged balls connected by 0.15 nm bonds.|Diamond and graphite are two](/wiki/File:Diamond_and_graphite2.jpg) [allotropes](/wiki/Allotrope) of carbon: pure forms of the same element that differ in structure.

A diamond is a [transparent](/wiki/Transparency_(optics)) [crystal](/wiki/Crystal) of [tetrahedrally](/wiki/Tetrahedral-octahedral_honeycomb) bonded carbon atoms in a covalent network lattice ([sp3](/wiki/Orbital_hybridisation)) that crystallizes into the [diamond lattice](/wiki/Diamond_cubic) which is a variation of the [face centered cubic](/wiki/Face_centered_cubic) structure. Diamonds have been adapted for many uses because of the material's exceptional physical characteristics. Most notable are its extreme hardness and thermal conductivity (900–[Template:Val](/wiki/Template:Val)),<ref name=PNU> [Template:Cite journal](/wiki/Template:Cite_journal)</ref> as well as wide [bandgap](/wiki/Bandgap) and high optical dispersion.<ref name=walker/> Above [Template:Val](/wiki/Template:Val) ([Template:Val](/wiki/Template:Val) / [Template:Val](/wiki/Template:Val)) in [vacuum](/wiki/Vacuum) or oxygen-free atmosphere, diamond converts to graphite; in air, transformation starts at ~[Template:Val](/wiki/Template:Val).[[11]](#cite_note-11) Diamond's ignition point is 720 – [Template:Val](/wiki/Template:Val) in oxygen and 850 – [Template:Val](/wiki/Template:Val) in air. Naturally occurring diamonds have a density ranging from 3.15–[Template:Val](/wiki/Template:Val), with pure diamond close to [Template:Val](/wiki/Template:Val).<ref name=mindat>[Template:Cite web](/wiki/Template:Cite_web)</ref> The chemical bonds that hold the carbon atoms in diamonds together are weaker than those in graphite. In diamonds, the bonds form an inflexible three-dimensional lattice, whereas in graphite, the atoms are tightly bonded into sheets, which can slide easily over one another, making the overall structure weaker.<ref name=Pop>[Template:Cite journal](/wiki/Template:Cite_journal)</ref> In a diamond, each carbon atom is surrounded by neighboring four carbon atoms forming a tetrahedral shaped unit.

### Hardness[[edit](/index.php?title=(none)&action=edit&section=7)]

Diamond is the hardest known natural material on both the [Vickers](/wiki/Vickers_hardness_test) and the [Mohs scale](/wiki/Mohs_scale_of_mineral_hardness). Diamond's hardness has been known since antiquity, and is the source of its name.

Diamond hardness depends on its purity, crystalline perfection and orientation: hardness is higher for flawless, pure crystals oriented to the [<111>](/wiki/Miller_index#Case_of_cubic_structures) direction (along the longest diagonal of the cubic diamond lattice).[[12]](#cite_note-12) Therefore, whereas it might be possible to scratch some diamonds with other materials, such as [boron nitride](/wiki/Boron_nitride), the hardest diamonds can only be scratched by other diamonds and [nanocrystalline diamond aggregates](/wiki/Aggregated_diamond_nanorod).

The hardness of diamond contributes to its suitability as a gemstone. Because it can only be scratched by other diamonds, it maintains its polish extremely well. Unlike many other gems, it is well-suited to daily wear because of its resistance to scratching—perhaps contributing to its popularity as the preferred gem in [engagement](/wiki/Engagement_ring) or [wedding rings](/wiki/Wedding_ring), which are often worn every day.

[thumb|The extreme hardness of diamond in certain orientations makes it useful in materials science, as in this pyramidal diamond embedded in the working surface of a](/wiki/File:Vickers_anvil_diamons.jpg) [Vickers hardness tester](/wiki/Vickers_hardness_test).

The hardest natural diamonds mostly originate from the [Copeton](/wiki/Copeton_Dam) and [Bingara](/wiki/Bingara) fields located in the [New England](/wiki/New_England_(Australia)) area in [New South Wales](/wiki/New_South_Wales), Australia. These diamonds are generally small, perfect to semiperfect octahedra, and are used to polish other diamonds. Their hardness is associated with the [crystal growth](/wiki/Crystal_growth) form, which is single-stage crystal growth. Most other diamonds show more evidence of multiple growth stages, which produce inclusions, flaws, and defect planes in the crystal lattice, all of which affect their hardness. It is possible to treat regular diamonds under a combination of high pressure and high temperature to produce diamonds that are harder than the diamonds used in hardness gauges.[[13]](#cite_note-13) Somewhat related to hardness is another mechanical property *toughness*, which is a material's ability to resist breakage from forceful impact. The [toughness](/wiki/Toughness) of natural diamond has been measured as 7.5–10 [MPa](/wiki/Megapascal)·m1/2.[[14]](#cite_note-14)[[15]](#cite_note-15) This value is good compared to other ceramic materials, but poor compared to most engineering materials such as engineering alloys, which typically exhibit toughnesses over 100 MPa·m1/2. As with any material, the macroscopic geometry of a diamond contributes to its resistance to breakage. Diamond has a [cleavage plane](/wiki/Cleavage_plane) and is therefore more fragile in some orientations than others. [Diamond cutters](/wiki/Diamond_cutting) use this attribute to cleave some stones, prior to faceting.<ref name=harlow/> "Impact toughness" is one of the main indexes to measure the quality of synthetic industrial diamonds.

### Pressure resistance[[edit](/index.php?title=(none)&action=edit&section=8)]

Used in so-called [diamond anvil](/wiki/Diamond_anvil) experiments to create high-pressure environments, diamonds are able to withstand crushing pressures in excess of 600 gigapascals (6 million [atmospheres](/wiki/Atmospheres)).[[16]](#cite_note-16)

### Electrical conductivity[[edit](/index.php?title=(none)&action=edit&section=9)]

Other specialized applications also exist or are being developed, including use as [semiconductors](/wiki/Semiconductor): some blue diamonds are natural semiconductors, in contrast to most diamonds, which are excellent [electrical insulators](/wiki/Insulator_(electricity)).[[17]](#cite_note-17) The conductivity and blue color originate from boron impurity. Boron substitutes for carbon atoms in the diamond lattice, donating a hole into the [valence band](/wiki/Valence_band).[[17]](#cite_note-17) Substantial conductivity is commonly observed in nominally [undoped](/wiki/Doping_(semiconductor)) diamond grown by [chemical vapor deposition](/wiki/Chemical_vapor_deposition_of_diamond). This conductivity is associated with hydrogen-related species adsorbed at the surface, and it can be removed by [annealing](/wiki/Annealing_(metallurgy)) or other surface treatments.[[18]](#cite_note-18)[[19]](#cite_note-19)

### Surface property[[edit](/index.php?title=(none)&action=edit&section=10)]

Diamonds are naturally [lipophilic](/wiki/Lipophilicity) and [hydrophobic](/wiki/Hydrophobe), which means the diamonds' surface cannot be wet by water but can be easily wet and stuck by oil. This property can be utilized to extract diamonds using oil when making synthetic diamonds. However, when diamond surfaces are chemically modified with certain ions, they are expected to become so [hydrophilic](/wiki/Hydrophile) that they can stabilize multiple layers of [water ice](/wiki/Ice) at [human body temperature](/wiki/Human_body_temperature).[[20]](#cite_note-20)

### Chemical stability[[edit](/index.php?title=(none)&action=edit&section=11)]

Diamonds are not very reactive. Under room temperature diamonds do not react with any chemical reagents including strong acids and bases. A diamond's surface can only be oxidized at temperatures above about [Template:Convert](/wiki/Template:Convert) in air. Diamond also reacts with fluorine gas above about [Template:Convert](/wiki/Template:Convert).

### Color[[edit](/index.php?title=(none)&action=edit&section=12)]

[Template:Main](/wiki/Template:Main) [alt=A museum display of jewelry items. Three brooches each consist of a large brown central gem surrounded by many clear small stones. A necklace has a large brown gem at its bottom and its string is all covered with small clear gems. A cluster-shaped decoration contains many brown gems.|300px|thumb|Brown diamonds at the](/wiki/File:National_Museum_of_Natural_History_Gold_Colored_Diamonds.JPG) [National Museum of Natural History](/wiki/National_Museum_of_Natural_History) in [Washington, D.C.](/wiki/Washington,_D.C.) [thumb|right|300px|alt=Picture of a diamond.|The most famous colored diamond,](/wiki/File:The_Hope_Diamond_-_SIA.jpg) [Hope Diamond](/wiki/Hope_Diamond) in 1974. Diamond has a wide [bandgap](/wiki/Bandgap) of [Template:Val](/wiki/Template:Val) corresponding to the deep [ultraviolet](/wiki/Ultraviolet) wavelength of 225 nanometers. This means pure diamond should transmit visible light and appear as a clear colorless crystal. Colors in diamond originate from lattice defects and impurities. The diamond crystal lattice is exceptionally strong and only atoms of nitrogen, boron and hydrogen can be introduced into diamond during the growth at significant concentrations (up to atomic percents). Transition metals nickel and cobalt, which are commonly used for growth of synthetic diamond by high-pressure high-temperature techniques, have been detected in diamond as individual atoms; the maximum concentration is 0.01% for nickel[[21]](#cite_note-21) and even less for cobalt. Virtually any element can be introduced to diamond by ion implantation.<ref name=zaitsev> [Template:Cite journal](/wiki/Template:Cite_journal)</ref>

Nitrogen is by far the most common impurity found in gem diamonds and is responsible for the yellow and brown color in diamonds. Boron is responsible for the blue color.<ref name=walker> [Template:Cite journal](/wiki/Template:Cite_journal)</ref> Color in diamond has two additional sources: irradiation (usually by alpha particles), that causes the color in green diamonds; and [plastic deformation](/wiki/Plastic_deformation) of the diamond crystal lattice. Plastic deformation is the cause of color in some brown[[22]](#cite_note-22) and perhaps pink and red diamonds.[[23]](#cite_note-23) In order of rarity, yellow diamond is followed by brown, colorless, then by blue, green, black, pink, orange, purple, and red.<ref name=harlow/> "Black", or [Carbonado](/wiki/Carbonado), diamonds are not truly black, but rather contain numerous dark inclusions that give the gems their dark appearance. Colored diamonds contain impurities or structural defects that cause the coloration, while pure or nearly pure diamonds are transparent and colorless. Most diamond impurities replace a carbon atom in the [crystal lattice](/wiki/Crystal_lattice), known as a [carbon flaw](/wiki/Carbon_flaw). The most common impurity, nitrogen, causes a slight to intense yellow coloration depending upon the type and concentration of nitrogen present.<ref name=harlow/> The [Gemological Institute of America](/wiki/Gemological_Institute_of_America) (GIA) classifies low saturation yellow and brown diamonds as diamonds in the *normal color range*, and applies a grading scale from "D" (colorless) to "Z" (light yellow). Diamonds of a different color, such as blue, are called *fancy colored* diamonds, and fall under a different grading scale.<ref name=harlow/>

In 2008, the [Wittelsbach Diamond](/wiki/Wittelsbach_Diamond), a [Template:Convert](/wiki/Template:Convert) blue diamond once belonging to the King of Spain, fetched over US$24 million at a Christie's auction.[[24]](#cite_note-24) In May 2009, a [Template:Convert](/wiki/Template:Convert) blue diamond fetched the highest price per carat ever paid for a diamond when it was sold at auction for 10.5 million Swiss francs (6.97 million euro or US$9.5 million at the time).[[25]](#cite_note-25) That record was however beaten the same year: a [Template:Convert](/wiki/Template:Convert) vivid pink diamond was sold for $10.8 million in Hong Kong on December 1, 2009.[[26]](#cite_note-26)

### Identification[[edit](/index.php?title=(none)&action=edit&section=13)]

Diamonds can be identified by their high thermal conductivity. Their high [refractive index](/wiki/Refractive_index) is also indicative, but other materials have similar refractivity. Diamonds cut glass, but this does not positively identify a diamond because other materials, such as quartz, also lie above glass on the [Mohs scale](/wiki/Mohs_scale) and can also cut it. Diamonds can scratch other diamonds, but this can result in damage to one or both stones. Hardness tests are infrequently used in practical gemology because of their potentially destructive nature.<ref name=read/> The extreme hardness and high value of diamond means that gems are typically polished slowly using painstaking traditional techniques and greater attention to detail than is the case with most other gemstones;<ref name=hazen>[Template:Cite book](/wiki/Template:Cite_book)</ref> these tend to result in extremely flat, highly polished facets with exceptionally sharp facet edges. Diamonds also possess an extremely high refractive index and fairly high dispersion. Taken together, these factors affect the overall appearance of a polished diamond and most diamantaires still rely upon skilled use of a [loupe](/wiki/Loupe) (magnifying glass) to identify diamonds 'by eye'.[[27]](#cite_note-27)

## Industry[[edit](/index.php?title=(none)&action=edit&section=14)]

[framed|alt=A clear faceted gem supported in four clamps attached to a wedding ring|A round](/wiki/File:Diamond.jpg) [brilliant cut](/wiki/Brilliant_(diamond_cut)) diamond set in a ring [Template:See also](/wiki/Template:See_also) The diamond industry can be separated into two distinct categories: one dealing with gem-grade diamonds and another for industrial-grade diamonds. Both markets value diamonds differently.

### Gem-grade diamonds[[edit](/index.php?title=(none)&action=edit&section=15)]

[Template:Main](/wiki/Template:Main) A large trade in gem-grade diamonds exists. Although most gem-grade diamonds are sold newly polished, there is a well-established market for resale of polished diamonds (e.g. pawnbroking, auctions, second-hand jewelry stores, diamantaires, bourses, etc.). One hallmark of the trade in gem-quality diamonds is its remarkable concentration: wholesale trade and diamond cutting is limited to just a few locations; in 2003, 92% of the world's diamonds were cut and polished in [Surat](/wiki/Surat), [India](/wiki/India).[[28]](#cite_note-28) Other important centers of diamond cutting and trading are the [Antwerp diamond district](/wiki/Antwerp_diamond_district) in [Belgium](/wiki/Belgium), where the [International Gemological Institute](/wiki/International_Gemological_Institute) is based, London, the [Diamond District](/wiki/Diamond_District) in New York City, the [Diamond Exchange District](/wiki/Diamond_Exchange_District) in [Tel Aviv](/wiki/Tel_Aviv), and Amsterdam. One contributory factor is the geological nature of diamond deposits: several large primary kimberlite-pipe mines each account for significant portions of market share (such as the [Jwaneng mine](/wiki/Jwaneng_diamond_mine) in Botswana, which is a single large-pit mine that can produce between [Template:Convert](/wiki/Template:Convert) to [Template:Convert](/wiki/Template:Convert) of diamonds per year[[29]](#cite_note-29)). Secondary alluvial diamond deposits, on the other hand, tend to be fragmented amongst many different operators because they can be dispersed over many hundreds of square kilometers (e.g., alluvial deposits in Brazil).

The production and distribution of diamonds is largely consolidated in the hands of a few key players, and concentrated in traditional diamond trading centers, the most important being Antwerp, where 80% of all rough diamonds, 50% of all cut diamonds and more than 50% of all rough, cut and industrial diamonds combined are handled.<ref name=India> [Template:Cite book](/wiki/Template:Cite_book)</ref> This makes Antwerp a de facto "world diamond capital".[[30]](#cite_note-30) The city of Antwerp also hosts the [Antwerpsche Diamantkring](/wiki/Antwerpsche_Diamantkring), created in 1929 to become the first and biggest diamond bourse dedicated to rough diamonds.[[31]](#cite_note-31) Another important diamond center is [New York City](/wiki/New_York_City), where almost 80% of the world's diamonds are sold, including auction sales.[[32]](#cite_note-32) The [De Beers](/wiki/De_Beers) company, as the world's largest diamond mining company, holds a dominant position in the industry, and has done so since soon after its founding in 1888 by the British imperialist [Cecil Rhodes](/wiki/Cecil_Rhodes). De Beers is currently the world's largest operator of diamond production facilities (mines) and [distribution channels](/wiki/Distribution_(business)) for gem-quality diamonds. The Diamond Trading Company (DTC) is a subsidiary of De Beers and markets rough diamonds from De Beers-operated mines. De Beers and its subsidiaries own mines that produce some 40% of annual world diamond production. For most of the 20th century over 80% of the world's rough diamonds passed through De Beers,[[33]](#cite_note-33) but by 2001–2009 the figure had decreased to around 45%,[[34]](#cite_note-34) and by 2013 the company's market share had further decreased to around 38% in value terms and even less by volume.[[35]](#cite_note-35) De Beers sold off the vast majority of its diamond stockpile in the late 1990s – early 2000s[[36]](#cite_note-36) and the remainder largely represents working stock (diamonds that are being sorted before sale).[[37]](#cite_note-37) This was well documented in the press[[38]](#cite_note-38) but remains little known to the general public.

As a part of reducing its influence, De Beers withdrew from purchasing diamonds on the open market in 1999 and ceased, at the end of 2008, purchasing Russian diamonds mined by the largest Russian diamond company [Alrosa](/wiki/Alrosa).[[39]](#cite_note-39) As of January 2011, De Beers states that it only sells diamonds from the following four countries: Botswana, Namibia, South Africa and Canada.[[40]](#cite_note-40) Alrosa had to suspend their sales in October 2008 due to the [global energy crisis](/wiki/2000s_energy_crisis),[[41]](#cite_note-41) but the company reported that it had resumed selling rough diamonds on the open market by October 2009.[[42]](#cite_note-42) Apart from Alrosa, other important diamond mining companies include [BHP Billiton](/wiki/BHP_Billiton), which is the world's largest mining company;[[43]](#cite_note-43) [Rio Tinto Group](/wiki/Rio_Tinto_Group), the owner of Argyle (100%), [Diavik](/wiki/Diavik_Diamond_Mine) (60%), and [Murowa](/wiki/Murowa_diamond_mine) (78%) diamond mines;[[44]](#cite_note-44) and [Petra Diamonds](/wiki/Petra_Diamonds), the owner of several major diamond mines in Africa. [thumb|right|Diamond polisher in Amsterdam](/wiki/File:Diamond_Polisher.jpg) Further down the supply chain, members of The [World Federation of Diamond Bourses](/wiki/World_Federation_of_Diamond_Bourses) (WFDB) act as a medium for wholesale diamond exchange, trading both polished and rough diamonds. The WFDB consists of independent diamond bourses in major cutting centers such as Tel Aviv, Antwerp, Johannesburg and other cities across the USA, Europe and Asia.<ref name=harlow/> In 2000, the WFDB and The International Diamond Manufacturers Association established the [World Diamond Council](/wiki/World_Diamond_Council) to prevent the trading of diamonds used to fund war and inhumane acts. WFDB's additional activities include sponsoring the [World Diamond Congress](/wiki/World_Diamond_Congress) every two years, as well as the establishment of the [*International Diamond Council*](/wiki/International_Diamond_Council) (IDC) to oversee diamond grading.

Once purchased by Sightholders (which is a trademark term referring to the companies that have a three-year supply contract with DTC), diamonds are cut and polished in preparation for sale as gemstones ('industrial' stones are regarded as a by-product of the gemstone market; they are used for abrasives).<ref name=polish>[Template:Cite book](/wiki/Template:Cite_book)</ref> The cutting and polishing of rough diamonds is a specialized skill that is concentrated in a limited number of locations worldwide.<ref name=polish/> Traditional diamond cutting centers are Antwerp, [Amsterdam](/wiki/Amsterdam), Johannesburg, New York City, and Tel Aviv. Recently, diamond cutting centers have been established in China, India, [Thailand](/wiki/Thailand), Namibia and Botswana.<ref name=polish/> Cutting centers with lower cost of labor, notably Surat in [Gujarat, India](/wiki/Gujarat), handle a larger number of smaller carat diamonds, while smaller quantities of larger or more valuable diamonds are more likely to be handled in Europe or North America. The recent expansion of this industry in India, employing low cost labor, has allowed smaller diamonds to be prepared as gems in greater quantities than was previously economically feasible.[[32]](#cite_note-32) Diamonds which have been prepared as gemstones are sold on diamond exchanges called *bourses*. There are 28 registered diamond bourses in the world.[[45]](#cite_note-45) Bourses are the final tightly controlled step in the diamond supply chain; wholesalers and even retailers are able to buy relatively small lots of diamonds at the bourses, after which they are prepared for final sale to the consumer. Diamonds can be sold already set in jewelry, or sold unset ("loose"). According to the Rio Tinto Group, in 2002 the diamonds produced and released to the market were valued at US$9 billion as rough diamonds, US$14 billion after being cut and polished, US$28 billion in wholesale diamond jewelry, and US$57 billion in retail sales.[[46]](#cite_note-46)

#### Cutting[[edit](/index.php?title=(none)&action=edit&section=16)]

[Template:Main](/wiki/Template:Main) [thumb|right|alt=A large rectangular pink multifaceted gemstone, set in a decorative surround. The decoration includes a row of small clear faceted gemstones around the main gem's perimeter, and clusters of gems forming a crest on one side. The crest comprises a three-pointed crown faced by two unidentifiable animals.|The](/wiki/File:The_Daria-e_Noor_(Sea_of_Light)_Diamond_from_the_collection_of_the_national_jewels_of_Iran_at_Central_Bank_of_Islamic_Republic_of_Iran.jpg) [Darya-I-Nur](/wiki/Darya-ye_Noor) Diamond—an example of unusual diamond cut and jewelry arrangement Mined rough diamonds are converted into gems through a multi-step process called "cutting". Diamonds are extremely hard, but also brittle and can be split up by a single blow. Therefore, diamond cutting is traditionally considered as a delicate procedure requiring skills, scientific knowledge, tools and experience. Its final goal is to produce a faceted jewel where the specific angles between the facets would optimize the diamond luster, that is dispersion of white light, whereas the number and area of facets would determine the weight of the final product. The weight reduction upon cutting is significant and can be of the order of 50%.<ref name=x50>[Template:Cite book](/wiki/Template:Cite_book)</ref> Several possible shapes are considered, but the final decision is often determined not only by scientific, but also practical considerations. For example, the diamond might be intended for display or for wear, in a ring or a necklace, singled or surrounded by other gems of certain color and shape.<ref name=antique>[Template:Cite book](/wiki/Template:Cite_book)</ref> Some of them may be considered as classical, such as [round](/wiki/Diamond_cut), [pear](/wiki/Pear_Cut_Diamond), [marquise](/wiki/Marquise_Diamond), [oval](/wiki/Oval_Cut_Diamond), [hearts and arrows](/wiki/Hearts_and_arrows) diamonds, etc. Some of them are special, produced by certain companies, for example, [Phoenix](/wiki/Phoenix_Cut_Diamond), [Cushion](/wiki/Cushion_Cut_Diamond), [Sole Mio](/wiki/Sole_Mio_Cut_Diamond) diamonds, etc.[[47]](#cite_note-47) The most time-consuming part of the cutting is the preliminary analysis of the rough stone. It needs to address a large number of issues, bears much responsibility, and therefore can last years in case of unique diamonds. The following issues are considered:

* The hardness of diamond and its ability to cleave strongly depend on the crystal orientation. Therefore, the crystallographic structure of the diamond to be cut is analyzed using [X-ray diffraction](/wiki/X-ray_diffraction) to choose the optimal cutting directions.
* Most diamonds contain visible non-diamond inclusions and crystal flaws. The cutter has to decide which flaws are to be removed by the cutting and which could be kept.
* The diamond can be split by a single, well calculated blow of a hammer to a pointed tool, which is quick, but risky. Alternatively, it can be cut with a [diamond saw](/wiki/Diamond_saw), which is a more reliable but tedious procedure.<ref name=antique/>[[48]](#cite_note-48)

After initial cutting, the diamond is shaped in numerous stages of polishing. Unlike cutting, which is a responsible but quick operation, polishing removes material by gradual erosion and is extremely time consuming. The associated technique is well developed; it is considered as a routine and can be performed by technicians.[[49]](#cite_note-49) After polishing, the diamond is reexamined for possible flaws, either remaining or induced by the process. Those flaws are concealed through various [diamond enhancement](/wiki/Diamond_enhancement) techniques, such as repolishing, crack filling, or clever arrangement of the stone in the jewelry. Remaining non-diamond inclusions are removed through laser drilling and filling of the voids produced.<ref name=read>[Template:Cite book](/wiki/Template:Cite_book)</ref>

#### Marketing[[edit](/index.php?title=(none)&action=edit&section=17)]

Marketing has significantly affected the image of diamond as a valuable commodity.

[N. W. Ayer & Son](/wiki/N._W._Ayer_&_Son), the advertising firm retained by [De Beers](/wiki/De_Beers) in the mid-20th century, succeeded in reviving the American diamond market. And the firm created new markets in countries where no diamond tradition had existed before. N. W. Ayer's marketing included [product placement](/wiki/Product_placement), advertising focused on the diamond product itself rather than the De Beers brand, and associations with celebrities and royalty. Without advertising the De Beers brand, De Beers was advertising its competitors' diamond products as well,[[50]](#cite_note-50) but this was not a concern as De Beers dominated the diamond market throughout the 20th century. De Beers' market share dipped temporarily to 2nd place in the global market below Alrosa in the aftermath of the global economic crisis of 2008, down to less than 29% in terms of carats mined, rather than sold.[[51]](#cite_note-51) The campaign lasted for decades but was effectively discontinued by early 2011. De Beers still advertises diamonds, but the advertising now mostly promotes its own brands, or licensed product lines, rather than completely "generic" diamond products.[[51]](#cite_note-51) The campaign was perhaps best captured by the slogan "a diamond is forever".[[52]](#cite_note-52) This slogan is now being used by De Beers Diamond Jewelers,[[53]](#cite_note-53) a jewelry firm which is a 50%/50% joint venture between the De Beers mining company and [LVMH](/wiki/LVMH), the luxury goods conglomerate.

Brown-colored diamonds constituted a significant part of the diamond production, and were predominantly used for industrial purposes. They were seen as worthless for jewelry (not even being assessed on the [diamond color](/wiki/Diamond_color) scale). After the development of Argyle diamond mine in Australia in 1986, and marketing, brown diamonds have become acceptable gems.[[54]](#cite_note-54)[[55]](#cite_note-55) The change was mostly due to the numbers: the Argyle mine, with its [Template:Convert](/wiki/Template:Convert) of diamonds per year, makes about one-third of global production of natural diamonds;[[56]](#cite_note-56) 80% of Argyle diamonds are brown.[[57]](#cite_note-57)

### Industrial-grade diamonds[[edit](/index.php?title=(none)&action=edit&section=18)]

[thumb|alt=A diamond scalpel consisting of a yellow diamond blade attached to a pen-shaped holder|A](/wiki/File:Dia_scalpel.jpg) [scalpel](/wiki/Scalpel) with synthetic diamond blade [thumb|alt=A polished metal blade embedded with small diamonds|Close-up photograph of an](/wiki/File:Diamond_blade_very_macro.jpg) [angle grinder](/wiki/Angle_grinder) blade with tiny diamonds shown embedded in the metal [thumb|A diamond knife blade used for cutting ultrathin sections (typically 70 to 350 nm) for transmission](/wiki/File:Diamond_Knife_Blade_Edge.jpg) [electron microscopy](/wiki/Electron_microscopy).

Industrial diamonds are valued mostly for their hardness and thermal conductivity, making many of the gemological characteristics of diamonds, such as the [4 Cs](/wiki/4_Cs), irrelevant for most applications. 80% of mined diamonds (equal to about [Template:Convert](/wiki/Template:Convert) annually), are unsuitable for use as gemstones, and used industrially.[[58]](#cite_note-58) In addition to mined diamonds, synthetic diamonds found industrial applications almost immediately after their invention in the 1950s; another [Template:Convert](/wiki/Template:Convert) of synthetic diamond is produced annually for industrial use (in 2004; in 2014 it's [Template:Convert](/wiki/Template:Convert), 90% of which is produced in China). Approximately 90% of diamond [grinding grit](/wiki/Grinding_(abrasive_cutting)) is currently of synthetic origin.<ref name=usgs> [Template:Cite web](/wiki/Template:Cite_web)</ref>

The boundary between gem-quality diamonds and industrial diamonds is poorly defined and partly depends on market conditions (for example, if demand for polished diamonds is high, some lower-grade stones will be polished into low-quality or small gemstones rather than being sold for industrial use). Within the category of industrial diamonds, there is a sub-category comprising the lowest-quality, mostly opaque stones, which are known as [bort](/wiki/Bort).<ref name=spear> [Template:Cite book](/wiki/Template:Cite_book)</ref>

Industrial use of diamonds has historically been associated with their hardness, which makes diamond the ideal material for cutting and grinding tools. As the hardest known naturally occurring material, diamond can be used to polish, cut, or wear away any material, including other diamonds. Common industrial applications of this property include diamond-tipped [drill bits](/wiki/Drill_bit) and saws, and the use of diamond powder as an [abrasive](/wiki/Abrasive). Less expensive industrial-grade diamonds, known as bort, with more flaws and poorer color than gems, are used for such purposes.[[59]](#cite_note-59) Diamond is not suitable for machining [ferrous](/wiki/Ferrous) [alloys](/wiki/Alloy) at high speeds, as carbon is soluble in iron at the high temperatures created by high-speed machining, leading to greatly increased wear on diamond tools compared to alternatives.[[60]](#cite_note-60) Specialized applications include use in laboratories as containment for [high pressure experiments](/wiki/Pressure_experiment) (see [diamond anvil cell](/wiki/Diamond_anvil_cell)), high-performance [bearings](/wiki/Bearing_(mechanical)), and limited use in specialized [windows](/wiki/Window).<ref name=spear/> With the continuing advances being made in the production of synthetic diamonds, future applications are becoming feasible. The high [thermal conductivity](/wiki/Thermal_conductivity) of diamond makes it suitable as a [heat sink](/wiki/Heat_sink) for integrated circuits in [electronics](/wiki/Electronics).[[61]](#cite_note-61)

### Mining[[edit](/index.php?title=(none)&action=edit&section=19)]

[Template:See also](/wiki/Template:See_also)

Approximately [Template:Convert](/wiki/Template:Convert) of diamonds are mined annually, with a total value of nearly US$9 billion, and about [Template:Convert](/wiki/Template:Convert) are synthesized annually.<ref name=yarnell> [Template:Cite journal](/wiki/Template:Cite_journal)</ref>

Roughly 49% of diamonds originate from [Central](/wiki/Central_Africa) and [Southern Africa](/wiki/Southern_Africa), although significant sources of the mineral have been discovered in [Canada](/wiki/Canada), [India](/wiki/India), [Russia](/wiki/Russia), [Brazil](/wiki/Brazil), and [Australia](/wiki/Australia).<ref name=usgs/> They are mined from kimberlite and lamproite volcanic pipes, which can bring diamond crystals, originating from deep within the Earth where high pressures and temperatures enable them to form, to the surface. The mining and distribution of natural diamonds are subjects of frequent controversy such as concerns over the sale of [*blood diamonds*](/wiki/Blood_diamond) or *conflict diamonds* by African [paramilitary](/wiki/Paramilitary) groups.<ref name=conflict> [Template:Cite web](/wiki/Template:Cite_web)</ref> The diamond supply chain is controlled by a limited number of powerful businesses, and is also highly concentrated in a small number of locations around the world.

Only a very small fraction of the diamond ore consists of actual diamonds. The ore is crushed, during which care is required not to destroy larger diamonds, and then sorted by density. Today, diamonds are located in the diamond-rich density fraction with the help of [X-ray fluorescence](/wiki/X-ray_fluorescence), after which the final sorting steps are done by hand. Before the use of [X-rays](/wiki/X-ray) became commonplace,<ref name=x50/> the separation was done with grease belts; diamonds have a stronger tendency to stick to grease than the other minerals in the ore.<ref name=harlow> [Template:Cite book](/wiki/Template:Cite_book)</ref> [thumb|](/wiki/File:Udachnaya_pipe.JPG)[Siberia's](/wiki/Siberia) Udachnaya diamond mine Historically, diamonds were found only in [alluvial deposits](/wiki/Alluvial_deposit) in [Guntur](/wiki/Guntur_district) and [Krishna district](/wiki/Krishna_district) of the [Krishna River](/wiki/Krishna_River) delta in [Southern India](/wiki/Southern_India).<ref name=Catelle1> [Template:Cite book](/wiki/Template:Cite_book)</ref> India led the world in diamond production from the time of their discovery in approximately the 9th century BC<ref name=hershey/><ref name=Ball> [Template:Cite book](/wiki/Template:Cite_book) Ball was a geologist in British service.</ref> to the mid-18th century AD, but the commercial potential of these sources had been exhausted by the late 18th century and at that time India was eclipsed by Brazil where the first non-Indian diamonds were found in 1725.<ref name=hershey/> Currently, one of the most prominent Indian mines is located at [Panna](/wiki/Panna_District).[[62]](#cite_note-62) Diamond extraction from primary deposits (kimberlites and lamproites) started in the 1870s after the discovery of the [Diamond Fields](/wiki/Diamond_Fields) in South Africa.[[63]](#cite_note-63)Production has increased over time and now an accumulated total of [Template:Convert](/wiki/Template:Convert) have been mined since that date.<ref name=giasummer2007> [Template:Cite journal](/wiki/Template:Cite_journal)</ref> Twenty percent of that amount has been mined in the last five years, and during the last 10 years, nine new mines have started production; four more are waiting to be opened soon. Most of these mines are located in Canada, Zimbabwe, Angola, and one in Russia.<ref name=giasummer2007/>

In the U.S., diamonds have been found in [Arkansas](/wiki/Arkansas), [Colorado](/wiki/Colorado), Wyoming, and [Montana](/wiki/Montana).<ref name=DGemGLorenz> [Template:Cite journal](/wiki/Template:Cite_journal)</ref><ref name=Montana> [Template:Cite web](/wiki/Template:Cite_web)</ref> In 2004, the discovery of a microscopic diamond in the U.S. led to the January 2008 bulk-sampling of [kimberlite pipes](/wiki/Kimberlite_pipes) in a remote part of Montana. The [Crater of Diamonds State Park](/wiki/Crater_of_Diamonds_State_Park) in [Arkansas](/wiki/Arkansas) is open to the public, and is the only mine in the world where members of the public can dig for diamonds.<ref name=Montana/>

Today, most commercially viable diamond deposits are in Russia (mostly in [Sakha Republic](/wiki/Sakha_Republic), for example [Mir pipe](/wiki/Mir_Mine) and [Udachnaya pipe](/wiki/Udachnaya_pipe)), [Botswana](/wiki/Botswana), Australia ([Northern](/wiki/Northern_Australia) and [Western Australia](/wiki/Western_Australia)) and the [Democratic Republic of the Congo](/wiki/Democratic_Republic_of_the_Congo).[[64]](#cite_note-64)In 2005, Russia produced almost one-fifth of the global diamond output, according to the [British Geological Survey](/wiki/British_Geological_Survey). Australia boasts the richest diamantiferous pipe, with production from the [Argyle diamond mine](/wiki/Argyle_diamond_mine) reaching peak levels of 42 metric tons per year in the 1990s.<ref name=DGemGLorenz/>[[65]](#cite_note-65)There are also commercial deposits being actively mined in the [Northwest Territories](/wiki/Northwest_Territories) of Canada and Brazil.<ref name=usgs/> Diamond prospectors continue to search the globe for diamond-bearing kimberlite and lamproite pipes.

### Political issues[[edit](/index.php?title=(none)&action=edit&section=20)]

[thumb|](/wiki/File:Unsustainable_Growth.webm)[Unsustainable diamond mining in Sierra Leone](http://en.wikibooks.org/wiki/Development_Cooperation_Handbook/Stories/Unsustainable_Growth)

[Template:Main](/wiki/Template:Main) In some of the more politically unstable central African and west African countries, revolutionary groups have taken control of [diamond mines](/wiki/List_of_diamond_mines), using proceeds from diamond sales to finance their operations. Diamonds sold through this process are known as *conflict diamonds* or *blood diamonds*.<ref name=conflict/> Major diamond trading corporations continue to fund and fuel these conflicts by doing business with armed groups.

In response to public concerns that their diamond purchases were contributing to war and [human rights abuses](/wiki/Human_rights_abuses) in [central](/wiki/Central_Africa) and [western](/wiki/West_Africa) Africa, the [United Nations](/wiki/United_Nations), the diamond industry and diamond-trading nations introduced the [Kimberley Process](/wiki/Kimberley_Process) in 2002.<ref name=kimb>[Template:Cite book](/wiki/Template:Cite_book)</ref> The Kimberley Process aims to ensure that conflict diamonds do not become intermixed with the diamonds not controlled by such rebel groups. This is done by requiring diamond-producing countries to provide proof that the money they make from selling the diamonds is not used to fund criminal or revolutionary activities. Although the Kimberley Process has been moderately successful in limiting the number of conflict diamonds entering the market, some still find their way in. According to the International Diamond Manufacturers Association, conflict diamonds constitute 2–3% of all diamonds traded.[[66]](#cite_note-66) Two major flaws still hinder the effectiveness of the Kimberley Process: (1) the relative ease of smuggling diamonds across African borders, and (2) the violent nature of diamond mining in nations that are not in a technical state of war and whose diamonds are therefore considered "clean".<ref name=kimb/>

The Canadian Government has set up a body known as the Canadian Diamond Code of Conduct[[67]](#cite_note-67) to help authenticate Canadian diamonds. This is a stringent tracking system of diamonds and helps protect the "conflict free" label of Canadian diamonds.[[68]](#cite_note-68)

## Synthetics, simulants, and enhancements[[edit](/index.php?title=(none)&action=edit&section=21)]

### Synthetics[[edit](/index.php?title=(none)&action=edit&section=22)]

[Template:Main](/wiki/Template:Main) [thumb|alt=Six crystals of cubo-octahedral shapes, each about 2 millimeters in diameter. Two are pale blue, one is pale yellow, one is green-blue, one is dark blue and one green-yellow.|Synthetic diamonds of various colors grown by the high-pressure high-temperature technique](/wiki/File:HPHTdiamonds2.JPG) Synthetic diamonds are diamonds manufactured in a laboratory, as opposed to diamonds mined from the Earth. The gemological and industrial uses of diamond have created a large demand for rough stones. This demand has been satisfied in large part by synthetic diamonds, which have been manufactured by various processes for more than half a century. However, in recent years it has become possible to produce gem-quality synthetic diamonds of significant size.[[6]](#cite_note-6) It is possible to make colorless synthetic gemstones that, on a molecular level, are identical to natural stones and so visually similar that only a gemologist with special equipment can tell the difference.[[69]](#cite_note-69) The majority of commercially available synthetic diamonds are yellow and are produced by so-called *high-pressure high-temperature* ([HPHT](/wiki/HPHT)) processes.[[70]](#cite_note-70) The yellow color is caused by [nitrogen](/wiki/Nitrogen) impurities. Other colors may also be reproduced such as blue, green or pink, which are a result of the addition of [boron](/wiki/Boron) or from [irradiation](/wiki/Irradiation) after synthesis.[[71]](#cite_note-71) [thumb|right|alt=A round, clear gemstone with many facets, the main face being hexagonal, surrounded by many smaller facets.|Colorless gem cut from diamond grown by chemical vapor deposition](/wiki/File:Apollo_synthetic_diamond.jpg) Another popular method of growing synthetic diamond is [chemical vapor deposition](/wiki/Chemical_vapor_deposition) (CVD). The growth occurs under low pressure (below atmospheric pressure). It involves feeding a mixture of gases (typically 1 to 99 [methane](/wiki/Methane) to [hydrogen](/wiki/Hydrogen)) into a chamber and splitting them to chemically active [radicals](/wiki/Radical_(chemistry)) in a [plasma](/wiki/Plasma_(physics)) ignited by [microwaves](/wiki/Microwaves), [hot filament](/wiki/Hot_filament), [arc discharge](/wiki/Electric_arc), [welding torch](/wiki/Welding_torch) or [laser](/wiki/Laser).<ref name=CVD> [Template:Cite journal](/wiki/Template:Cite_journal)</ref> This method is mostly used for coatings, but can also produce single crystals several millimeters in size (see picture).<ref name=yarnell/>

As of 2010, nearly all 5,000 million carats (1,000 tonnes) of synthetic diamonds produced per year are for industrial use. Around 50% of the 133 million carats of natural diamonds mined per year end up in industrial use.[[69]](#cite_note-69)[[72]](#cite_note-72) Mining companies' expenses average $40 to $60 per carat for natural colorless diamonds, while synthetic manufacturers' expenses average $2,500 per carat for synthetic, gem-quality colorless diamonds.[[69]](#cite_note-69)[Template:Rp](/wiki/Template:Rp) However, a purchaser is more likely to encounter a synthetic when looking for a fancy-colored diamond because nearly all synthetic diamonds are fancy-colored, while only 0.01% of natural diamonds are.[[73]](#cite_note-73)

### Simulants[[edit](/index.php?title=(none)&action=edit&section=23)]

[Template:Main](/wiki/Template:Main) [thumb|alt=A round sparkling, clear gemstone with many facets.|Gem-cut synthetic silicon carbide set in a ring](/wiki/File:Moissanite_ring.JPG) A diamond simulant is a non-diamond material that is used to simulate the appearance of a diamond, and may be referred to as diamante. [Cubic zirconia](/wiki/Cubic_zirconia) is the most common. The gemstone [moissanite](/wiki/Moissanite) (silicon carbide) can be treated as a diamond simulant, though more costly to produce than cubic zirconia. Both are produced synthetically.[[74]](#cite_note-74)

### Enhancements[[edit](/index.php?title=(none)&action=edit&section=24)]

[Template:Main](/wiki/Template:Main) Diamond enhancements are specific treatments performed on natural or synthetic diamonds (usually those already cut and polished into a gem), which are designed to better the gemological characteristics of the stone in one or more ways. These include laser drilling to remove inclusions, application of sealants to fill cracks, treatments to improve a white diamond's color grade, and treatments to give fancy color to a white diamond.[[75]](#cite_note-75) Coatings are increasingly used to give a diamond simulant such as cubic zirconia a more "diamond-like" appearance. One such substance is [diamond-like carbon](/wiki/Diamond-like_carbon)—an amorphous carbonaceous material that has some physical properties similar to those of the diamond. Advertising suggests that such a coating would transfer some of these diamond-like properties to the coated stone, hence enhancing the diamond simulant. Techniques such as [Raman spectroscopy](/wiki/Raman_spectroscopy) should easily identify such a treatment.[[76]](#cite_note-76)

### Identification[[edit](/index.php?title=(none)&action=edit&section=25)]

Early diamond identification tests included a scratch test relying on the superior hardness of diamond. This test is destructive, as a diamond can scratch another diamond, and is rarely used nowadays. Instead, diamond identification relies on its superior thermal conductivity. Electronic thermal probes are widely used in the gemological centers to separate diamonds from their imitations. These probes consist of a pair of battery-powered [thermistors](/wiki/Thermistor) mounted in a fine copper tip. One thermistor functions as a heating device while the other measures the temperature of the copper tip: if the stone being tested is a diamond, it will conduct the tip's thermal energy rapidly enough to produce a measurable temperature drop. This test takes about 2–3 seconds.[[77]](#cite_note-77) Whereas the thermal probe can separate diamonds from most of their simulants, distinguishing between various types of diamond, for example synthetic or natural, irradiated or non-irradiated, etc., requires more advanced, optical techniques. Those techniques are also used for some diamonds simulants, such as silicon carbide, which pass the thermal conductivity test. Optical techniques can distinguish between natural diamonds and synthetic diamonds. They can also identify the vast majority of treated natural diamonds.<ref name=raman>[Template:Cite book](/wiki/Template:Cite_book)</ref> "Perfect" crystals (at the atomic lattice level) have never been found, so both natural and synthetic diamonds always possess characteristic imperfections, arising from the circumstances of their crystal growth, that allow them to be distinguished from each other.<ref name=spot/>

Laboratories use techniques such as spectroscopy, microscopy and luminescence under shortwave ultraviolet light to determine a diamond's origin.<ref name=raman/> They also use specially made instruments to aid them in the identification process. Two screening instruments are the *DiamondSure* and the *DiamondView*, both produced by the [DTC](/wiki/Diamond_Trading_Company) and marketed by the GIA.[[78]](#cite_note-78) Several methods for identifying synthetic diamonds can be performed, depending on the method of production and the color of the diamond. CVD diamonds can usually be identified by an orange fluorescence. D-J colored diamonds can be screened through the [Swiss Gemmological Institute's](/wiki/Swiss_Gemmological_Institute)[[79]](#cite_note-79) Diamond Spotter. Stones in the D-Z color range can be examined through the DiamondSure UV/visible spectrometer, a tool developed by De Beers.<ref name=spot> [Template:Cite journal](/wiki/Template:Cite_journal)</ref> Similarly, natural diamonds usually have minor imperfections and flaws, such as inclusions of foreign material, that are not seen in synthetic diamonds.

Screening devices based on diamond type detection can be used to make a distinction between diamonds that are certainly natural and diamonds that are potentially synthetic. Those potentially synthetic diamonds require more investigation in a specialized lab. Examples of commercial screening devices are D-Screen (WTOCD / HRD Antwerp) and Alpha Diamond Analyzer (Bruker / HRD Antwerp).

## Stolen diamonds[[edit](/index.php?title=(none)&action=edit&section=26)]

Occasionally large thefts of diamonds take place. In February 2013 armed robbers carried out a raid at [Brussels Airport](/wiki/Brussels_Airport) and escaped with gems estimated to be worth $50m (£32m; 37m euros). The gang broke through a perimeter fence and raided the cargo hold of a Swiss-bound plane. The gang have since been arrested and large amounts of cash and diamonds recovered.[[80]](#cite_note-80) The identification of stolen diamonds presents a set of difficult problems. Rough diamonds will have a distinctive shape depending on whether their source is a mine or from an alluvial environment such as a beach or river - alluvial diamonds have smoother surfaces than those that have been mined. Determining the provenance of cut and polished stones is much more complex.

The [Kimberley Process](/wiki/Kimberley_Process) was developed to monitor the trade in rough diamonds and prevent their being used to fund violence. Before exporting, rough diamonds are certificated by the government of the country of origin. Some countries, such as Venezuela, are not party to the agreement. The Kimberley Process does not apply to local sales of rough diamonds within a country.

Diamonds may be etched by laser with marks invisible to the naked eye. [Lazare Kaplan](/wiki/Lazare_Kaplan_International), a US-based company, developed this method. However, whatever is marked on a diamond can readily be removed.[[81]](#cite_note-81)[[82]](#cite_note-82)

## See also[[edit](/index.php?title=(none)&action=edit&section=27)]

[Template:Portal](/wiki/Template:Portal)

* [List of diamonds](/wiki/List_of_diamonds)
  + [List of largest rough diamonds](/wiki/List_of_largest_rough_diamonds)
* [List of minerals](/wiki/List_of_minerals)
* [Diamonds on Jupiter and Saturn](/wiki/Diamonds_on_Jupiter_and_Saturn) [Lonsdaleite](/wiki/Lonsdaleite)

## References[[edit](/index.php?title=(none)&action=edit&section=28)]

[Template:Reflist](/wiki/Template:Reflist)

## Books[[edit](/index.php?title=(none)&action=edit&section=29)]

* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)
* [Template:Cite book](/wiki/Template:Cite_book)

## External links[[edit](/index.php?title=(none)&action=edit&section=30)]

[Template:Sister project links](/wiki/Template:Sister_project_links)

* [Properties of diamond: Ioffe database](http://www.ioffe.ru/SVA/NSM/Semicond/Diamond/index.html)
* ["A Contribution to the Understanding of Blue Fluorescence on the Appearance of Diamonds"](http://lgdl.gia.edu/pdfs/W97_fluoresce.pdf). (2007) Gemological Institute of America (GIA)
* Tyson, Peter (November 2000). ["Diamonds in the Sky"](http://www.pbs.org/wgbh/nova/diamond/sky.html). Retrieved March 10, 2005.
* [Have You Ever Tried to Sell a Diamond?](http://www.theatlantic.com/doc/198202/diamond)

[Template:Allotropes of carbon](/wiki/Template:Allotropes_of_carbon) [Template:Jewellery](/wiki/Template:Jewellery) [Template:Authority control](/wiki/Template:Authority_control)

[Template:Featured article](/wiki/Template:Featured_article)

[Category:Diamond](/wiki/Category:Diamond) [Category:Abrasives](/wiki/Category:Abrasives) [Category:Articles containing video clips](/wiki/Category:Articles_containing_video_clips) [Category:Cubic minerals](/wiki/Category:Cubic_minerals) [Category:Economic geology](/wiki/Category:Economic_geology) [Category:Impact event minerals](/wiki/Category:Impact_event_minerals) [Category:Native element minerals](/wiki/Category:Native_element_minerals) [Category:Group IV semiconductors](/wiki/Category:Group_IV_semiconductors) [Category:Transparent materials](/wiki/Category:Transparent_materials) [Category:Luminescent minerals](/wiki/Category:Luminescent_minerals)